# las2txt

Converts from binary LAS/LAZ 1.0 - 1.4 to an ASCII text format.

The '-sep space' flag specifies what separator to use. The
default is a space but 'tab', 'comma', 'colon', 'hyphen',
'dot', or 'semicolon' are other possibilities.

The '-header pound' flag results in the header information
being printed at the beginning of the ASCII file in form of
a comment that starts with the special character '#'. Also
possible are 'percent', 'dollar', 'comma', 'star',
'colon', or 'semicolon' as that special character.
 

## Examples

    las2txt64 -i *.laz -parse xyzit -sep comma

converts all LAZ files to ASCII files and places the
x, y, and z coordinate of each point as the 1st, 2nd, and 3rd
entries, the intensity as the 4th entry, and the gps_time as the
5th entry of each line. The output files containing a first line 
with the column description to enable automatic reconversion using txt2las64.


    las2txt64 -i lidar.las -o lidar.txt -parse xyz

converts LAS file to ASCII and places the x, y, and z coordinate
of each point at the 1st, 2nd, and 3rd entry of each line. the
entries are separated by a space.


    las2txt64 -i lidar.laz -o lidar.txt -parse xyzEit -extra 0.1

converts LAZ file to ASCII and places the x, y, and z coordinate
of each point at the 1st, 2nd, and 3rd entry of each line. the
extra string "0.1" as the 4th entry and the intensity and time
of each point as the 5th and 6th entry.


    las2txt64 -i lidar_1_3.las -o lidar.txt -parse WV

converts LAS 1.3 file including waveform information to ASCII. it
places the wavepacket info of each point followed by its entire
waveform into one line separated by spaces.


    las2txt64 -i lidar.laz -o lidar.txt -parse txyzr -sep comma

converts LAZ file to ASCII and places the gps_time as the first
entry, the x, y, and z coordinates at the 2nd, 3rd, and 4th entry
and the number of the return as the 5th entry of each line. the
entries are separated by a comma.

 
    las2txt64 -i lidar.laz -o lidar.txt -parse xyzRGB

converts LAZ file to ASCII and places the x, y, and z coordinates
at the 1st, 2nd, and 3rd entry and the r, g, and b value of the
RGB color as the 4th, 5th, and 6th entry of each line. the entries
are separated by a space. note that lidar.las should be format 1.2
or higher (because 1.0 and 1.1 do not support RGB colors).


    las2txt64 -i lidar.las -o lidar.txt -parse xyzia -sep semicolon -header pound

converts LAS file to ASCII and places the x, y, and z coordinate
at the 1st, 2nd, and 3rd entry, the intensity at the 4th and the
scan angle as the 5th entry of each line. the entries are separated
by a semicolon. at the beginning of the file we print the header
information as a comment starting with a '#' symbol.


    las2txt64 -i lidar.laz -o lidar.txt -parse xyzcu -sep tab -header percent

converts LAZ file to ASCII and places the x, y, and z coordinate
at the 1st, 2nd, and 3rd entry, the classification at the 4th and
the user data as the 5th entry of each line. the entries are
separated by a semicolon. at the beginning of the file we print
the header information as a comment starting with a '%' symbol.


    las2txt64 -i lidar.las -o lidar.txt -parse ko

extracts only the 'k'eypoint and the 'o'verlap flags of each LiDAR
points into an ASCII file. Note that the overlap flag exists only
for LAS/LAZ files containing the LAS 1.4 point types 6 or higher. 


las2txt -h  
las2txt -i test.las -parse Mxyzrna -stdout | more  
las2txt -i *.las -parse xyzt  
las2txt -i flight1*.las flight2*.las -parse xyziarn  
las2txt -i *.las -parse xyzrn -sep comma -verbose  
las2txt -i lidar.las -parse xyztE -extra 99 -o ascii.txt


## las2txt specific arguments

-extra [n]   : use [n] as value of output extra string  
-header [n]  : use header prefix [n] (pound,percent,dollar,comma,star,colon,semicolon)  
-opts        : output as PTS (plain text lidar data)  
-optx        : output as PTX (plain text with header)  
-parse [xyz] : use parse string [xyz] to access point values  
-parse_all   : set "txyzirndecaup" as parse string to parse all available information  
-sep [n]     : output separator [comma,space,semicolon,tab,colon,hyphen,dot], (default=space)  
-coldesc     : write a header line to the output containing the column description  
               (this enables to omit -parse during import using txt2las)

### Basics
-cores [n]      : process multiple inputs on [n] cores in parallel  
-h, -help       : print help output  
-v, -verbose    : verbose output (print extra information)  
-vv             : very verbose output (print even more information)  
-silent         : only output on errors or warnings  
-quiet          : no output at all  
-force          : continue, even if serious warnings occur  
-errors_ignore  : continue, even if errors occur (if possible). Use with caution!  
-print_log_stats: print additional log statistics  
-cpu64          : force 32bit version to start 64 bit in multi core (obsolete)  
-gui            : start with files loaded into GUI  
-version        : reports this tool's version number  


## Module arguments

### General
-comma_not_point   : use comma instead of point as decimal separator  
-chunk_size [n]    : set chunk size [n] in number of bytes  
-neighbors [n]     : set neighbors filename or wildcard [n]  
-neighbors_lof [n] : set neighbors list of files [fnf]  
-stored            : use in memory reader  

### Color
-clamp_RGB_to_8bit                  : limit RGB values to 8 bit (otherwise: 16 bit)  
-copy_B_into_NIR                    : copy blue color value into NearInfraRed value  
-copy_B_into_intensity              : copy blue color value to intensity  
-copy_B_into_register [n]           : copy blue color value into register [n]  
-copy_G_into_NIR                    : copy green color value into NearInfraRed value  
-copy_G_into_intensity              : copy green color value to intensity  
-copy_G_into_register [n]           : copy green color value into register [n]  
-copy_NIR_into_intensity            : copy NIR into intensity  
-copy_NIR_into_register [n]         : copy NearInfraRed value into register [n]  
-copy_RGB_into_intensity            : copy weighted RGB value to intensity  
-copy_R_into_NIR                    : copy red color value into NearInfraRed value  
-copy_R_into_intensity              : copy red color value to intensity  
-copy_R_into_register [n]           : copy red color value into register [n]  
-copy_attribute_into_B [n]          : copy attribute [n] value into blue  
-copy_attribute_into_G [n]          : copy attribute [n] value into green  
-copy_attribute_into_NIR [n]        : copy attribute [n] value into NIR (NearInfraRed)  
-copy_attribute_into_R [n]          : copy attribute [n] value into red  
-copy_intensity_into_NIR            : copy intensity into NIR (NearInfraRed) value  
-copy_register_into_B [n]           : copy register [n] into blue color value  
-copy_register_into_G [n]           : copy register [n] into green color value  
-copy_register_into_I [n]           : copy register [n] into NearInfraRed value  
-copy_register_into_NIR [n]         : copy register [n] into NearInfraRed value  
-copy_register_into_R [n]           : copy register [n] into red color value  
-drop_RGB_green [min] [max]         : drop points with green color value between [min] and [max]  
-drop_RGB_red [min] [max]           : drop points with red color value between [min] and [max]  
-force_RGB                          : force the use of the RGB value even if the point format does not support RGB  
-keep_NDVI [min] [max]              : keep NDVI (Normalized Difference Vegetation Index) between [min] [max]  
-keep_NDVI_from_CIR [min] [max]     : keep NDVI (Normalized Difference Vegetation Index) from CIR between [min] [max]  
-keep_NDVI_green_is_NIR [min] [max] : keep NDVI (Normalized Difference Vegetation Index) where green is NIR between [min] [max]  
-keep_NDVI_blue_is_NIR [min] [max]  : keep NDVI (Normalized Difference Vegetation Index) where blue is NIR between [min] [max]  
-keep_NDVI_intensity_is_NIR [min] [max]: keep NDVI (Normalized Difference Vegetation Index) where intensity is NIR between [min] [max]  
-keep_RGB_blue [m] [n]              : keep points with RGB blue color values between [min] [max]  
-keep_RGB_green [min] [max]         : keep points with green color value between [min] and [max]  
-keep_RGB_greenness [m] [n]         : keep points with RGB greenness values between [min] [max]  
-keep_RGB_nir [m] [n]               : keep points with RGB NIR values between [min] [max]  
-keep_RGB_red [min] [max]           : keep points with red color value between [min] and [max]  
-map_attribute_into_RGB [a] [fnm]   : map attribute [a] by table in file [fnm] to RGB values  
-oscale_rgb [n]                     : scale output RGB by [n]  
-scale_NIR [n]                      : scale NearInfraRed value by factor [n]  
-scale_NIR_down                     : scale NearInfraRed value down by 256  
-scale_NIR_to_16bit                 : scale 8 bit NearInfraRed value to 16 bit  
-scale_NIR_to_8bit                  : scale 16 bit NearInfraRed value downto 8 bit  
-scale_NIR_up                       : scale NearInfraRed value up by 256  
-scale_RGB [r] [g] [b]              : scale RGB values by factors in [r][g][b]  
-scale_RGB_down                     : scale RGB color values down by 256  
-scale_RGB_to_16bit                 : scale 8 bit color values to 16 bit  
-scale_RGB_to_8bit                  : scale 16 bit color values downto 8 bit  
-scale_RGB_up                       : scale RGB values from 8 bit up to 16 bit (multiply with 256)  
-scale_rgb_down                     : divides all RGB values by 256 (to go from 16 bit to 8 bit numbers)  
-scale_rgb_up                       : multiplies all RGB values by 256 (to go from 8 bit to 16 bit numbers)  
-set_NIR [n]                        : set NearInfraRed value to [n]  
-set_RGB [r] [g] [b]                : set color to [r] [g] [b]  
-set_RGB_of_class [c] [r] [g] [b]   : set RGB values of class [c] to [r][g][b] (8 or 16 bit)  
-switch_G_B                         : switch green and blue value  
-switch_RGBI_into_CIR               : set R to NIR; G to R; B to G  
-switch_RGB_intensity_into_CIR      : set R to intensity; G to R; B to G  
-switch_R_B                         : switch red and blue color value  
-switch_R_G                         : switch red and green color value  
-keep_HSV [hmin] [hmax] [smin] [smax] [vmin] [vmax] : keep only points with RGB values of HSV color range  
-keep_HSV_hue [hmin] [hmax]         : keep points with RGB values of HSV hue color range  
-keep_HSV_saturation [smin] [smax]  : keep points with RGB values of HSV saturation color range  
-keep_HSV_value [vmin] [vmax]       : keep points with RGB values of HSV value color range  
-drop_HSV_hue [hmin] [hmax]         : drop points with RGB values of HSV hue color range  
-drop_HSV_saturation [smin] [smax]  : drop points with RGB values of HSV saturation color range  
-drop_HSV_value [vmin] [vmax]       : drop points with RGB values of HSV value color range  
-keep_HSL [hmin] [hmax] [smin] [smax] [lmin] [lmax] : keep only points with RGB values of HSL hue color range  
-keep_HSL_hue [hmin] [hmax]         : keep points with RGB values of HSL hue color range  
-keep_HSL_saturation [smin] [smax]  : keep points with RGB values of HSL saturation color range  
-keep_HSL_lightness [lmin] [lmax]   : keep points with RGB values of HSL lightness color range  
-drop_HSL_hue [hmin] [hmax]         : drop points with RGB values of HSL hue color range  
-drop_HSL_saturation [smin] [smax]  : drop points with RGB values of HSL saturation color range  
-drop_HSL_lightness [lmin] [lmax]   : drop points with RGB values of HSL lightness color range  


### Coordinates
-add_attribute_to_z [n]             : add value of attribute [n] to z value  
-add_scaled_attribute_to_z [m] [n]  : scale attribute [m] value by [n] and add to z value  
-auto_reoffset                      : puts a reasonable offset in the header and translates the points accordingly. Only applicable to LAS/LAZ input files  
-bin_Z_into_point_source [n]        : set point source to z/[n]  
-clamp_raw_z [min] [max]            : limit raw z values to [min] and [max]  
-clamp_z [min] [max]                : limit z values to [min] and [max]  
-clamp_z_above [n]                  : limit z values to maximal [n]  
-clamp_z_below [n]                  : limit z values to minimal [n]  
-classify_z_above_as [m] [n]        : for z value above [m] set class to [n]  
-classify_z_below_as [m] [n]        : for z value below [m] set class to [n]  
-classify_z_between_as [m] [n] [o]  : for z value between [m] and [n] set class to [o]  
-copy_attribute_into_x [n]          : copy attribute [n] value into x  
-copy_attribute_into_y [n]          : copy attribute [n] value into y  
-copy_attribute_into_z [n]          : copy attribute [n] value into z  
-copy_intensity_into_z              : copy intensity to z value  
-copy_register_into_x [n]           : copy register [n] to x value  
-copy_register_into_y [n]           : copy register [n] to y value  
-copy_register_into_z [n]           : copy register [n] to z value  
-copy_user_data_into_z              : copy user data into z  
-copy_z_into_attribute [n]          : copy z value into attribute [n] value  
-drop_x [m] [n]                     : drop points with x value between [m] and [n]  
-drop_x_above [n]                   : drop points with x value above [n]  
-drop_x_below [n]                   : drop points with x value below [n]  
-drop_xy [x1] [y1] [x2] [y2]        : drop points within the [x1] [y1] [x2] [y2] rectangle  
-drop_xyz [x1] [y1] [z1] [x2] [y2] [z2]: drop points within the given cube dimensions  
-drop_y [m] [n]                     : drop points with y value between [m] and [n]  
-drop_y_above [n]                   : drop points with y value above [n]  
-drop_y_below [n]                   : drop points with y value below [n]  
-drop_z [m] [n]                     : drop points with z value between [m] and [n]  
-drop_z_above [n]                   : drop points with z value above [n]  
-drop_z_below [n]                   : drop points with z value below [n]  
-inside [x1] [y1] [x2] [y2]         : use only points within the [x1] [y1] [x2] [y2] rectangle  
-inside_circle [x] [y] [r]          : keep circle at pos [x] [y] with radius [r]  
-inside_rectangle [x1] [y1] [x2] [y2]: use only points within the [x1] [y1] [x2] [y2] rectangle  
-inside_tile [m] [n] [o]            : use only points inside tile at lower-left [x] [y] with size [s]  
-keep_circle [x] [y] [r]            : keep circle at pos [x] [y] with radius [r]  
-keep_profile [x1] [y1] [x2] [y2] [w]: keep profile with [x1] [y1] [x2] [y2] [w]  
-keep_tile [x] [y] [size]           : keep tile at lower-left [x] [y] with size [s]  
-keep_x [m] [n]                     : keep points with x value between [m] and [n]  
-keep_xy [x1] [y1] [x2] [y2]        : keep points within the [x1] [y1] [x2] [y2] rectangle  
-keep_xyz [x1] [y1] [z1] [x2] [y2] [z2]: keep points within the given cube dimensions  
-keep_y [m] [n]                     : keep points with y value between [m] and [n]  
-keep_z [m] [n]                     : keep points with z value between [m] and [n]  
-keep_z_above [n]                   : keep points with z value above [n]  
-keep_z_below [n]                   : keep points with z value below [n]  
-offset_adjust                      : adjusting the offset based on the results of point operations and transformations  
-reoffset [x] [y] [z]               : puts a new offset [x] [y] [z] into the header and translates the points accordingly  
-rescale [x] [y] [z]                : puts a new scale [x] [y] [z] into the header and rescales the points accordingly  
-rescale_xy [x] [y]                 : rescale x y by [x] [y]  
-rescale_z [z]                      : rescale z by [z]  
-rotate_xy [a] [x] [y]              : rotate points by [a] degrees, center at [x] [y]  
-rotate_xz [a] [x] [z]              : rotate points by [a] degrees, center at [x] [z]  
-rotate_yz [a] [y] [z]              : rotate points by [a] degrees, center at [y] [z]  
-scale_x [n]                        : scale x value by [n]  
-scale_xyz [m] [n] [o]              : scale xyz values by [m] [n] [o]  
-scale_y [n]                        : scale y value by [n]  
-scale_z [n]                        : scale z value by [n]  
-switch_x_y                         : exchange x and y value  
-switch_x_z                         : exchange x and z value  
-switch_y_z                         : exchange z and x value  
-transform_affine [k,w,x,y]         : transform by k*cos(w)+k*sin(w)+tx;k*cos(w)+k*sin(w)+ty - angle in second of arc  
-transform_helmert [m] [n] [o]      : do a helmert transformation with 3 or 7 comma separated parameters [n] ...  
-transform_matrix [r11,r12,r13] [r21,r22,r23] [r31,r32,r33] [tr1,tr2,tr3]: transform input using matrix [r11,r12,r13] [r21,r22,r23] [r31,r32,r33] [tr1,tr2,tr3]  
-translate_raw_x [n]                : translate raw x value by [n]  
-translate_raw_xy_at_random [x] [y] : translate raw xy values by random and max offset of [x] [y]  
-translate_raw_xyz [x] [y] [z]      : translate raw coordinates by [x] [y] [z]  
-translate_raw_y [n]                : translate raw y value by [n]  
-translate_raw_z [n]                : translate raw z value by [n]  
-translate_scale_translate_x [m] [n]: calculate x value as (x–[m])*[n]+[m]  
-translate_scale_translate_y [m] [n]: calculate y value as (y–[m])*[n]+[m]  
-translate_scale_translate_z [m] [n]: calculate z value as (z–[m])*[n]+[m]  
-translate_then_scale_x [m] [n]     : translate x value by [m] and scale by [n]  
-translate_then_scale_y [m] [n]     : translate y value by [m] and scale by [n]  
-translate_then_scale_z [m] [n]     : translate z value by [m] and scale by [n]  
-translate_x [n]                    : translate y value by [n]  
-translate_xyz [x] [y] [z]          : translate point coordinates by [x] [y] [z]  
-translate_y [n]                    : translate y value by [n]  
-translate_z [n]                    : translate z value by [n]  

### Simple thinning
-drop_every_nth [n]           : drop every [n]th point  
-keep_every_nth [n]           : keep every [n]th point  
-keep_random_fraction [m] [n] : keep points by random fraction [m]{0-1}, optional seed [n]  
-thin_points_with_time [n]    : thin points with time, [n] = timespacing  
-thin_pulses_with_time [n]    : thin pulses with time, [n] = timespacing  
-thin_with_grid [n]           : thin points by min grid size of [n]  
-thin_with_time [n]           : thin pulses with time, [n] = timespacing  

### Return number
-change_extended_number_of_returns_from_to [m] [n]: change extended number of returns from [m] to [n]  
-change_extended_return_number_from_to [m] [n]: change extended return number from [m] to [n]  
-change_number_of_returns_from_to [m] [n]: change number of returns from [m] to [n]  
-change_return_number_from_to [m] [n]: change return number from [m] to [n]  
-drop_double                        : drop double returns  
-drop_first                         : drop first return  
-drop_first_of_many                 : drop first of many returns  
-drop_last                          : drop last return  
-drop_last_of_many                  : drop last of many returns  
-drop_middle                        : drop middle returns  
-drop_number_of_returns [n]         : drop points with [n] number of returns  
-drop_quadruple                     : drop quadruple returns  
-drop_quintuple                     : drop quintuple returns  
-drop_return [m] [n]...             : drop points with return [m] [n]...  
-drop_return_mask [n]               : drop points with return mask [n]  
-drop_second_last                   : drop points with second last return  
-drop_single                        : drop points with single return  
-drop_triple                        : drop points with triple return  
-first_only                         : use first return only  
-keep_double                        : keep double returns  
-keep_first                         : keep first return  
-keep_first_of_many                 : keep first of many returns  
-keep_last                          : keep last return  
-keep_last_of_many                  : keep last of many returns  
-keep_middle                        : keep mittle returns  
-keep_number_of_returns [n]         : keep points with [n] number of returns  
-keep_quadruple                     : keep quadruple returns  
-keep_quintuple                     : keep quintuple returns  
-keep_return [m] [n]...             : keep points with return [m] [n]...  
-keep_return_mask [n]               : keep points with return mask [n]  
-keep_second_last                   : keep points with second last return  
-keep_single                        : keep points with single return  
-keep_triple                        : keep points with triple return  
-last_only                          : use last return only  
-repair_zero_returns                : sets return counts and number of returns that are zero to one  
-set_extended_number_of_returns [n] : set extended number of returns to [n]  
-set_extended_return_number [n]     : set extended return number to [n]  
-set_number_of_returns [n]          : set number of returns to [n]  
-set_return_number [n]              : set return number to [n]  

### Scanline
-drop_scan_direction [n]       : drop points with scan direction [n]  
-faf                           : input files are flightlines. do ***NOT*** use this for tiled input  
-faf_index [n]                 : set files are flightlines index [n]  
-files_are_flightlines         : input files are flightlines. do ***NOT*** use this for tiled input  
-drop_edge_of_flight_line      : drop points with "Edge of Flight Line" flag set  
-keep_edge_of_flight_line      : keep points with "Edge of Flight Line" flag set  
-keep_scan_direction_change    : keep points with changed scan direction flag  
-set_edge_of_flight_line [0/1] : set "Edge of Flight Line" flag to [0/1]  
-set_scan_direction_flag [0/1] : set scan direction flag to [0/1]  

### Scanner channel
-copy_scanner_channel_into_point_source: copy scanner channel into point_source  
-copy_scanner_channel_into_user_data: copy scanner channel into user data  
-copy_user_data_into_scanner_channel: copy user data into scanner channel  
-drop_scanner_channel [n]           : drop points with scanner channel [n]  
-keep_scanner_channel [n]           : keep points with scanner channel [n]  
-merge_scanner_channel_into_point_source: merge scanner channel to point source  
-set_extended_scanner_channel [n]   : set extended scanner channel to [n]  
-set_scanner_channel [n]            : set scanner channel to [n]  
-split_scanner_channel_from_point_source: split scanner channel from point source and save as extended scanner channel  

### Source ID
-apply_file_source_ID               : copy file source ID to target  
-bin_Z_into_point_source [n]        : set point source to z/[n]  
-bin_abs_scan_angle_into_point_source [n]: set point source to scan_angle/[n]  
-bin_gps_time_into_point_source [n] : set point source to gps/[n]  
-change_point_source_from_to [m] [n]: change point source from [m] to [n]  
-copy_attribute_into_point_source [n]: copy attribute [n] value into point source  
-copy_classification_into_point_source: copy classification to point source  
-copy_point_source_into_register [n]: copy point source into register [n]  
-copy_register_into_point_source [n]: copy register [n] to point source  
-copy_scanner_channel_into_point_source: copy scanner channel into point_source  
-copy_user_data_into_point_source   : copy user data into point source  
-drop_point_source [n]              : drop points with point source [n]  
-drop_point_source_above [n]        : drop points with with point source above [n]  
-drop_point_source_below [n]        : drop points with with point source below [n]  
-drop_point_source_between [m] [n]  : drop points with with point source between [n] and [m]  
-keep_point_source [n]              : keep points with point source [n]  
-keep_point_source_between [m] [n]  : keep points with with point source between [n] and [m]  
-map_point_source [fnm]             : set the point source by map in file [fnm]  
-merge_scanner_channel_into_point_source: merge scanner channel to point source  
-set_point_source [n]               : set point source to [n]  
-split_scanner_channel_from_point_source: split scanner channel from point source and save as extended scanner channel  

### User data
-add_scaled_attribute_to_user_data [m] [n]: scale attribute [m] value by [n] and add to user data  
-change_user_data_from_to [m] [n]   : change user data from [m] to [n]  
-copy_attribute_into_user_data [n]  : copy attribute [n] value into user data field  
-copy_classification_into_user_data : copy classification to user data  
-copy_register_into_user_data [n]   : copy register [n] to user data  
-copy_scanner_channel_into_user_data: copy scanner channel into user data  
-copy_user_data_into_attribute [n]  : copy user data into attribute [n] value  
-copy_user_data_into_classification : copy user data into classification  
-copy_user_data_into_point_source   : copy user data into point source  
-copy_user_data_into_register [n]   : copy user data to register [n]  
-copy_user_data_into_scanner_channel: copy user data into scanner channel  
-copy_user_data_into_z              : copy user data into z  
-drop_user_data [n]                 : drop points with user data value of [n]  
-drop_user_data_above [n]           : drop points with user data value above [n]  
-drop_user_data_below [n]           : drop points with user data value below [n]  
-drop_user_data_between [m] [n]     : drop points with user data between [m] and [n]  
-keep_user_data [n]                 : keep points with user data value of [n]  
-keep_user_data_above [n]           : keep points with user data value above [n]  
-keep_user_data_below [n]           : keep points with user data value below [n]  
-keep_user_data_between [m] [n]     : keep points with user data between [m] and [n]  
-map_user_data [fnm]                : set the user data by map in file [fnm]  
-scale_user_data [n]                : scale user data by [n]  
-set_user_data [n]                  : sets all user_data fields to [n]  

### Classification
-change_class_from_to [m] [n]       : change classification from [m] to [n]  
-change_classification_from_to [m] [n]: change classification from [m] to [n]  
-change_extended_class_from_to [m] [n]: change extended class from [m] to [n]  
-change_extended_classification_from_to [m] [n]: change extended class from [m] to [n]  
-classify_attribute_above_as [m] [n] [o]: for attribute [m] with value above [n] set class to [o]  
-classify_attribute_below_as [m] [n] [o]: for attribute [m] with value below [n] set class to [o]  
-classify_attribute_between_as [m] [n] [o] [p]: for attribute [m] with value between [n] and [o] set class to [p]  
-classify_intensity_above_as [m] [n]: for intensity value above [m] set class to [n]  
-classify_intensity_below_as [m] [n]: for intensity value below [m] set class to [n]  
-classify_intensity_between_as [m] [n] [o]: for intensity value between [m] and [n] set class to [o]  
-classify_z_above_as [m] [n]        : for z value above [m] set class to [n]  
-classify_z_below_as [m] [n]        : for z value below [m] set class to [n]  
-classify_z_between_as [m] [n] [o]  : for z value between [m] and [n] set class to [o]  
-copy_classification_into_point_source: copy classification to point source  
-copy_classification_into_user_data : copy classification to user data  
-copy_intensity_into_classification : copy intensity to classification  
-copy_user_data_into_classification : copy user data into classification  
-drop_class [m] [n] [o]...          : drop points with class in [m][n][o]...  
-drop_classification [m] [n] [o]... : drop points with class in [m][n][o]...  
-drop_classification_mask [n]       : drop points with classification mask matches [n]  
-drop_extended_class [m] [n]...     : drop extended class [m] [n]...  
-drop_extended_classification [n]   : drop points with extended classification [n]  
-drop_extended_classification_mask [a] [b] [c] [d] [e] [f] [g] [h]: drop points with extended classification mask matches [a] [b] [c] [d] [e] [f] [g] [h]  
-keep_class [m] [n] [o]...          : keep points with class in [m][n][o]...  
-keep_classification [m] [n] [o]... : keep points with class in [m][n][o]...  
-keep_classification_mask [n]       : keep points with classification mask matches [n]  
-keep_extended_class [m] [n]...     : keep extended class [m] [n]...  
-keep_extended_classification [n]   : keep points with extended class [n]  
-move_ancient_to_extended_classification: move old data to extended classification  
-set_RGB_of_class [c] [r] [g] [b]   : set RGB values of class [c] to [r][g][b] (8 or 16 bit)  
-set_classification [n]             : set classification to [n]  
-set_extended_classification [n]    : set extended classification to [n]  

### Extra byte
-add_attribute_to_z [n]             : add value of attribute [n] to z value  
-add_scaled_attribute_to_user_data [m] [n]: scale attribute [m] value by [n] and add to user data  
-add_scaled_attribute_to_z [m] [n]  : scale attribute [m] value by [n] and add to z value  
-classify_attribute_above_as [m] [n] [o]: for attribute [m] with value above [n] set class to [o]  
-classify_attribute_below_as [m] [n] [o]: for attribute [m] with value below [n] set class to [o]  
-classify_attribute_between_as [m] [n] [o] [p]: for attribute [m] with value between [n] and [o] set class to [p]  
-copy_attribute_into_B [n]          : copy attribute [n] value into blue  
-copy_attribute_into_G [n]          : copy attribute [n] value into green  
-copy_attribute_into_I [n]          : copy attribute [n] value into intensity  
-copy_attribute_into_NIR [n]        : copy attribute [n] value into NIR (NearInfraRed)  
-copy_attribute_into_R [n]          : copy attribute [n] value into red  
-copy_attribute_into_intensity [n]  : copy attribute [n] value into intensity  
-copy_attribute_into_point_source [n]: copy attribute [n] value into point source  
-copy_attribute_into_register [m] [n]: copy attribute [m] value into register [m]  
-copy_attribute_into_user_data [n]  : copy attribute [n] value into user data field  
-copy_attribute_into_x [n]          : copy attribute [n] value into x  
-copy_attribute_into_y [n]          : copy attribute [n] value into y  
-copy_attribute_into_z [n]          : copy attribute [n] value into z  
-copy_intensity_into_attribute [n]  : copy intensity to attribute [n] value  
-copy_register_into_attribute [m] [n]: copy register [m] to attribute [n] value  
-copy_user_data_into_attribute [n]  : copy user data into attribute [n] value  
-copy_z_into_attribute [n]          : copy z value into attribute [n] value  
-drop_attribute_above [m] [n]       : drop points with attribute [m] value > [n]  
-drop_attribute_below [m] [n]       : drop points with attribute [m] value < [n]  
-drop_attribute_between [m] [n] [o] : drop points with attribute [m] in range [n]...[o]  
-iadd_attribute [m] [n] [o] [p] [q] [r] [s] [t]: adds a new "extra_byte" attribute of data_type [m] name [n] description [o]; optional: scale[p] offset [q] pre_scale [r] pre_offset [s] no_data_value [t]  
-iadd_extra [m] [n] [o] [p] [q] [r] [s] [t]: adds a new "extra_byte" attribute of data_type [m] name [n] description [o]; optional: scale[p] offset [q] pre_scale [r] pre_offset [s] no_data_value [t]  
-keep_attribute_above [m] [n]       : keep points with attribute [m] value > [n]  
-keep_attribute_below [m] [n]       : keep points with attribute [m] value < [n]  
-keep_attribute_between [m] [n] [o] : keep points with attribute [m] in range [n]...[o]  
-load_attribute_from_text [m] [fnt] : load attribute [m] from file [fnt]  
-map_attribute_into_RGB [a] [fnm]   : map attribute [a] by table in file [fnm] to RGB values  
-scale_attribute [m] [n]            : scale attribute [m] by [n]  
-set_attribute [m] [n]              : set attribute [m] with value [n]  
-translate_attribute [m] [n]        : translate attribute [n] by [n]  

### Flags
-drop_keypoint                   : drop points flaged as keypoint  
-drop_overlap                    : drop points flaged as overlap  
-drop_scan_direction [n]         : drop points with scan direction [n]  
-drop_synthetic                  : drop points flaged as synthetic  
-drop_withheld                   : drop points flaged as withheld  
-keep_edge_of_flight_line        : keep points with "Edge of Flight Line" flag set  
-keep_keypoint                   : keep points flaged as keypoint  
-keep_overlap                    : keep points flaged as overlap  
-keep_scan_direction_change      : keep points with changed scan direction flag  
-keep_synthetic                  : keep points flaged as synthetic  
-keep_withheld                   : keep points flaged as withheld  
-set_edge_of_flight_line [0/1]   : set "Edge of Flight Line" flag to [0/1]  
-set_extended_overlap_flag [0/1] : set extended overlap flag to [0/1]  
-set_keypoint_flag [0/1]         : set keypoint flag to [0/1]  
-set_overlap_flag [0/1]          : set overlap flag to [0/1]  
-set_scan_direction_flag [0/1]   : set scan direction flag to [0/1]  
-set_synthetic_flag [0/1]        : set synthetic flag to [0/1]  
-set_withheld_flag [0/1]         : set withheld flag to [0/1]  

### GPS time
-adjusted_to_week                   : converts time stamps from Adjusted Standard GPS to GPS week  
-bin_gps_time_into_intensity [n]    : set intensity time to gps/[n]  
-bin_gps_time_into_point_source [n] : set point source to gps/[n]  
-drop_gps_time_above [n]            : drop points with GPS time above [n]  
-drop_gps_time_below [n]            : drop points with GPS time below [n]  
-drop_gps_time_between [m] [n]      : drop points with GPS time between [m] and [n]  
-drop_gpstime_above [n]             : drop points with GPS time above [n]  
-drop_gpstime_below [n]             : drop points with GPS time below [n]  
-drop_gpstime_between [m] [n]       : drop points with GPS time between [m] and [n]  
-keep_gps_time [m] [n]              : keep points with GPS time between [m] and [n]  
-keep_gps_time_above [n]            : keep points with GPS time above [n]  
-keep_gps_time_below [n]            : keep points with GPS time below [n]  
-keep_gps_time_between [m] [n]      : keep points with GPS time between [m] and [n]  
-keep_gpstime [m] [n]               : keep points with GPS time between [m] and [n]  
-keep_gpstime_above [n]             : keep points with GPS time above [n]  
-keep_gpstime_below [n]             : keep points with GPS time below [n]  
-keep_gpstime_between [m] [n]       : keep points with GPS time between [m] and [n]  
-set_gps_time [n]                   : set gps time to [n]  
-translate_gps_time [n]             : translate GPS time by [n]  
-week_to_adjusted [n]               : converts time stamps from GPS week [n] to Adjusted Standard GPS  

### Intensity
-bin_gps_time_into_intensity [n]    : set intensity time to gps/[n]  
-clamp_intensity [min] [max]        : limit intensity values to [min] and [max]  
-clamp_intensity_above [max]        : limit intensity values to maximal [max]  
-clamp_intensity_below [max]        : limit intensity values to minimal [min]  
-classify_intensity_above_as [m] [n]: for intensity value above [m] set class to [n]  
-classify_intensity_below_as [m] [n]: for intensity value below [m] set class to [n]  
-classify_intensity_between_as [m] [n] [o]: for intensity value between [m] and [n] set class to [o]  
-copy_B_into_intensity              : copy blue color value to intensity  
-copy_G_into_intensity              : copy green color value to intensity  
-copy_NIR_into_intensity            : copy NIR into intensity  
-copy_RGB_into_intensity            : copy weighted RGB value to intensity  
-copy_R_into_intensity              : copy red color value to intensity  
-copy_attribute_into_I [n]          : copy attribute [n] value into intensity  
-copy_attribute_into_intensity [n]  : copy attribute [n] value into intensity  
-copy_intensity_into_NIR            : copy intensity into NIR (NearInfraRed) value  
-copy_intensity_into_attribute [n]  : copy intensity to attribute [n] value  
-copy_intensity_into_classification : copy intensity to classification  
-copy_intensity_into_register [n]   : copy color intensitiy value into register [n]  
-copy_intensity_into_z              : copy intensity to z value  
-copy_register_into_intensity [n]   : copy register [n] into point intensitiy value  
-drop_intensity_above [n]           : drop points with intensity value above [n]  
-drop_intensity_below [n]           : drop points with intensity value below [n]  
-drop_intensity_between [m] [n]     : drop points with intensity value between [m] and [n]  
-iscale_intensity [n]               : scale intensity value by [n]  
-itranslate_intensity [n]           : translate input intensity by [n]  
-keep_NDVI_intensity_is_NIR [min] [max]: keep NDVI (Normalized Difference Vegetation Index) where intensity is NIR between [min] [max]  
-keep_intensity [m] [n]             : keep points with intensity between [m] and [n]  
-keep_intensity_above [n]           : keep points with intensity value above [n]  
-keep_intensity_below [n]           : keep points with intensity value below [n]  
-map_intensity [fnm]                : set the intensity by map in file [fnm]  
-scale_intensity [n]                : multiply intensity by [n]  
-set_intensity [n]                  : set intensity to [n]  
-switch_RGB_intensity_into_CIR      : set R to intensity; G to R; B to G  
-translate_intensity [n]            : translate intensity by [n]  
-translate_then_scale_intensity [m] [n]: translate intensity by [m] and scale by [n]  

### Raw point values
-clamp_raw_z [min] [max]            : limit raw z values to [min] and [max]  
-translate_raw_x [n]                : translate raw x value by [n]  
-translate_raw_xy_at_random [x] [y] : translate raw xy values by random and max offset of [x] [y]  
-translate_raw_xyz [x] [y] [z]      : translate raw coordinates by [x] [y] [z]  
-translate_raw_y [n]                : translate raw y value by [n]  
-translate_raw_z [n]                : translate raw z value by [n]  

### Registers
-add_registers [m] [n] [o]          : add register [m] and [n] and store result in register [o]  
-copy_B_into_register [n]           : copy blue color value into register [n]  
-copy_G_into_register [n]           : copy green color value into register [n]  
-copy_NIR_into_register [n]         : copy NearInfraRed value into register [n]  
-copy_R_into_register [n]           : copy red color value into register [n]  
-copy_attribute_into_register [m] [n]: copy attribute [m] value into register [m]  
-copy_intensity_into_register [n]   : copy color intensitiy value into register [n]  
-copy_point_source_into_register [n]: copy point source into register [n]  
-copy_register_into_B [n]           : copy register [n] into blue color value  
-copy_register_into_G [n]           : copy register [n] into green color value  
-copy_register_into_I [n]           : copy register [n] into NearInfraRed value  
-copy_register_into_NIR [n]         : copy register [n] into NearInfraRed value  
-copy_register_into_R [n]           : copy register [n] into red color value  
-copy_register_into_attribute [m] [n]: copy register [m] to attribute [n] value  
-copy_register_into_intensity [n]   : copy register [n] into point intensitiy value  
-copy_register_into_point_source [n]: copy register [n] to point source  
-copy_register_into_user_data [n]   : copy register [n] to user data  
-copy_register_into_x [n]           : copy register [n] to x value  
-copy_register_into_y [n]           : copy register [n] to y value  
-copy_register_into_z [n]           : copy register [n] to z value  
-copy_user_data_into_register [n]   : copy user data to register [n]  
-divide_registers [m] [n] [o]       : divide register [m] by register [n] and store result in register [o]  
-multiply_registers [m] [n] [o]     : Multiply register [m] with [n] and store result in register [o]  
-scale_register [m] [n]             : scale register index [m] with factor [n]  
-set_register [m] [n]               : set register [m] with value [n]  
-subtract_registers [m] [n] [o]     : subtract register [m] by register [n] and store result in register [o]  
-translate_register [m] [n]         : translate register index [m] value by [n]  

### Scan angle
-bin_abs_scan_angle_into_point_source [n]: set point source to scan_angle/[n]  
-drop_abs_scan_angle_above [max]    : drop points with absolute scan angle above [max]  
-drop_abs_scan_angle_below [min]    : drop points with absolute scan angle below [min]  
-drop_scan_angle_above [n]          : drop points with scan angle above [n]  
-drop_scan_angle_below [n]          : drop points with scan angle below [n]  
-drop_scan_angle_between [m] [n]    : drop points with scan angle between [m] and [n]  
-iscale_scan_angle [n]              : scale scan angle by [n]  
-itranslate_scan_angle [n]          : translate input scan angle by [n]  
-keep_scan_angle [m] [n]            : keep points with scan angle between [m] and [n]  
-keep_scan_angle_between [m] [n]    : keep points with scan angle between [m] and [n]  
-scale_scan_angle [n]               : scale scan angle by [n]  
-set_scan_angle [n]                 : set scan angle to [n]  
-translate_scan_angle [n]           : translate scan angle by [n]  
-translate_then_scale_scan_angle [m] [n]: translate scan angle by [m] and scale by [n]  

### Tiles
-keep_tile [x] [y] [size] : keep tile at lower-left [x] [y] with size [s]  

### Waveform packet
-drop_wavepacket [n]     : drop points with wavepacket value of [n]  
-flip_waveform_direction : flip the waveform direction in the waveform VLR  
-keep_wavepacket [n]     : keep points with wavepacket value of [n]  

### Logical
-filter_and         : boolean AND combination of last 2 filters  
-filter_or          : boolean OR combination of last 2 filters  
-filtered_transform : do the transformation only on points of the current filter  

### Input
-i [fnp]        : input file or input file mask [fnp] (e.g. *.laz;fo?.la?;esri.shp,...)  
-io_ibuffer [n] : use read-input-buffer of size [n] bytes  
-iparse [xyz]   : define fields [xyz] for text input parser  
-ipts           : input as PTS (plain text lidar source), store header in VLR  
-iptx           : input as PTX (plain text extended lidar data), store header in VLR  
-iptx_transform : use PTX file header to transform point data  
-iskip [n]      : skip [n] lines at the beginning of the text input  
-itxt           : expect input as text file  
-lof [fnf]      : use input out of a list of files [fnf]  
-unique         : remove duplicate files in a -lof list  
-merged         : merge input files  
-buffered [n]   : use on-the-fly buffering of size [n] for tiles without implicit buffer  
-stdin          : pipe from stdin  

### Output
-compatible      : write LAS/LAZ output in compatibility mode  
-do_not_populate : do not populate header on output  
-io_obuffer [n]  : use write-out-buffer of size [n] bytes  
-native          : write LAS/LAZ output in native/actual mode  
-nil             : pipe output to NULL (suppress output)  
-o [n]           : use [n] as output file  
-obin            : output as BIN (terrasolid binary)  
-ocut [n]        : cut the last [n] characters from name  
-odir [n]        : set output directory to [n]  
-odix [n]        : set output file name suffix to [n]  
-oforce          : force output creation also on errors or warnings  
-olas            : output as LAS file  
-olaz            : output as LAZ (compressed LAS)  
-oparse [xyz]    : parse on-the-fly to ASCII using fields [xyz]  
-oqi             : output in QFIT format (.qi)(ATM project, NASA)  
-oscale_rgb [n]  : scale output RGB by [n]  
-osep [sep]      : set text output separator as [sep](see table below)  
-otxt            : output as textfile  
-owrl            : output as VRLM (Virtual Reality Modeling Language) text  
-pipe_on         : write output to command pipe, see also -std_in  
-populate        : populate header on output  
-stdout          : pipe to stdout  
-temp_files [n]  : set base file name [n] for temp files (example: E:\tmp)  

### parse
The '-parse [xyz]' flag specifies how to interpret each line of the ASCII file.
For example, 'tsxyzssa' means that the first number is the gpstime, the next
number should be skipped, the next three numbers are the x, y, and z coordinate,
the next two should be skipped, and the next number is the scan angle.

The other supported entries are:  
    x : [x] coordinate  
    y : [y] coordinate  
    z : [z] coordinate  
    X : unscaled raw [X] value   
    Y : unscaled raw [Y] value  
    Z : unscaled raw [Z] value  
    t : gps [t]ime  
    R : RGB [R]ed channel  
    G : RGB [G]reen channel  
    B : RGB [B]lue channel  
    I : N[I]R channel of LAS 1.4 point type 8  
    i : [i]ntensity  
    a : scan [a]ngle  
    n : [n]umber of returns of that given pulse  
    r : number of [r]eturn  
    h : with[h]eld flag  
    k : [k]eypoint flag  
    g : synthetic fla[g]  
    o : [o]verlap flag of LAS 1.4 point types 6, 7, 8  
    l : scanner channe[l] of LAS 1.4 point types 6, 7, 8  
    c : [c]lassification. If extended classes are used: Use o,l or I to force 1.4 format.  
    u : [u]ser data  
    p : [p]oint source ID  
    e : [e]dge of flight line flag  
    d : [d]irection of scan flag  
    0-9 : additional attributes described as extra bytes (0 through 9)  
    (13) : additional attributes described as extra bytes (10 and up)  
    m : point index, starting at 0  
    M : point index, starting at 1  
    w : [w]avepacket descriptor index  
    W : all wavepacket attributes  
    _ : diff of unscaled raw integer X to prev point  
    ! : diff of unscaled raw integer Y to prev point  
    @ : diff of unscaled raw integer Z to prev point  
    # : diff of gps-time to prev point  
    $ : R difference to the last point  
    & : the byte-wise R difference to the last point  
    % : the G difference to the last point  
    * : the byte-wise G difference to the last point  
    ^ : the B difference to the last point  
    + : the byte-wise B difference to the last point  
    V : the waveform data  
    E : extra string (-extra)  
 (HSV): color in HSV model [0,360|100]. Converted from RGB.  
 (HSL): color in HSL model [0,360|100]. Converted from RGB.  
 (hsv): color in HSV model [0,1]. Converted from RGB.  
 (hsl): color in HSL model [0,1]. Converted from RGB.  

### column descriptions
If argument '-coldesc' is given a header row with the column description
will be generated:  

  Column description  Corresponding parse character  
  x                   x coordinate  
  y                   y coordinate  
  z                   z coordinate  
  X                   X (unscaled raw X value)  
  Y                   Y (unscaled raw Y value)  
  Z                   Z (unscaled raw Z value)  
  gps_time            t (gps time)  
  intensity           i   
  scan_angle          a  
  point_source_id     p  
  classification      c  
  user_data           u  
  return_number       r  
  number_of_returns   n  
  edge_of_flight_line e  
  scan_direction_flag d  
  withheld_flag       h  
  keypoint_flag       k  
  synthetic_flag      g  
  skip                s (skip this column without warning)  
  overlap_flag        o  
  scanner_channel     l  
  R                   R (RGB red)  
  G                   G (RGB green)  
  B                   B (RGB blue)  
  HSV_H               (HSV) HSV color model hue [0..360]  
  HSV_S                                     saturation [0..100]  
  HSV_V                                     value [0..100]  
  HSV_h               (hsv) HSV color model hue [0..1]  
  HSV_s                                     saturation [0..1]  
  HSV_v                                     value [0..1]   
  HSL_H               (HSL) HSL color model hue [0..360]  
  HSL_S                                     saturation [0..100]  
  HSL_L                                     luminance [0..100]   
  HSL_h               (hsl) HSL color model hue [0..1]  
  HSL_s                                     saturation [0..1]  
  HSL_l                                     luminance [0..1]  


### output separator
The '-osep [sep]' argument specifies the output format of a text(xyz) output.  
Supported [sep] values:  

  comma  
  tab  
  dot  
  colon  
  semicolon  
  hyphen  
  space  

## Licensing

This tool is free to use.

## Support

1. We invite you to join our LAStools Google Group (http://groups.google.com/group/lastools/).
   If you are looking for information about a specific tool, enter the tool name in the search 
   function and you'll find all discussions related to the respective tool. 
2. Customer Support Page: https://rapidlasso.de/customer-support/.  
3. Download LAStools: https://rapidlasso.de/downloads/.  
4. Changelog: https://rapidlasso.de/changelog/.  


If you want to send us feedback or have questions that are not answered in the resources above, 
please email to info@rapidlasso.de.
